Squeezeplay for Joggler                                                                      birdslikewires.co.uk
USB Installer v1.03 (17th April 2012)

-----------------------

WARNING! No responsibility will be accepted for any loss or damage
         which occurs through the use of these files. This software
         is provided without warranty.

If you find SqueezePlay for Joggler useful, you might like to make a contribution
towards it's hosting and development. For more information, please visit:

http://birdslikewires.co.uk/about/donate

-----------------------

This will install SqueezePlay on an O2 Joggler running the default operating system.

Please ensure that you are running software version 26635.S3 (June 25 2010) before using this.


Instructions
------------

1. Copy the contents of the zip file to a FAT16 or FAT32 formatted USB stick.
2. Make sure you have copied all the files, including the '.sum' file.
3. Plug the USB stick into a powered-off Joggler.
4. Power on the Joggler and wait until the normal interface appears.

When the script has completed, your Joggler should beep twice.

Once finished, you should find a SqueezePlay icon on your screen. Please be aware that your Joggler's interface will restart during this process and the screen may be blank for up to 30 seconds; this is expected behaviour, so don't panic.


Troubleshooting
---------------

- Make sure that you are running software version 26635.S3 (June 25 2010)
  You can check using the Settings app and choosing 'About'.

- Make sure you copied the '.sum' file to your USB stick.
  This is a hidden file on UNIX-based systems.

- No beeps? It may be that everything finished before the audio system was activated. Just give it a try!


Version History
---------------
v1.03 (17th April 2012)
Tweaked opupdt.run to set execute bit, in case I forget.
Updated to squeezeplay-joggler-v141.tgz.
Updated to squeezeplay-thinned-7.7.2-9704.tgz.
Updated to sqpinstall.sh v1.11.

v1.02 (16th April 2012)
Minor tweaks to the installation script.

v1.00 (15th April 2012)
First version that worked properly.

